|  |
| --- |
|  |
| **Interface Control Document**  Systems Engineering**-Company E** |
| **COP** |
| Prepared for: |
| Anders Jacob Truelsen (Systematic)  By: Anders Torndahl, Christian Jensen, David Neergaard Rasmussen Marmoy, Michael Nygaard Pedersen, Peter Høgh Mikkelsen |
|  |
|  |

|  |  |
| --- | --- |
|  | |
| System requirement specification | |
| Project: | $System Engineering**– Company E** |
| Revision: | $Revision: 1A$ $Date:08102010$ |
| Document: | $ |
| Copyright (c) 2010 by Systematic Group. It shall not be copied, reproduced, disclosed or otherwise made available to third party without previous consent from Systematic Group | |

Table of Contents

[1 Introduction 1](#_Toc274146111)

[2 Interface design 1](#_Toc274146112)

[2.1 Interface identification and diagrams 1](#_Toc274146113)

[2.2 CCRT and CCRC Interface 2](#_Toc274146114)

[2.2.1 Type of interface 2](#_Toc274146115)

[2.2.2 Interface data elements and setup 3](#_Toc274146116)

[2.2.3 Address bus 3](#_Toc274146117)

[2.2.4 Data bus 3](#_Toc274146118)

[2.2.5 Memory Map 3](#_Toc274146119)

[2.2.6 Control registers 3](#_Toc274146120)

[2.2.7 Status registers 3](#_Toc274146121)

[2.2.8 Data registers 3](#_Toc274146122)

[2.2.9 Hardware characteristics 3](#_Toc274146123)

[3 Bibliography 4](#_Toc274146124)

# Introduction

This document describes the analysis process on the case work with the Common Operations Picture (COP) case from Systematic. Company E is the main contractor and this document will explain one of the critical interfaces involved.

# Interface design

This paragraph describes the interface characteristics of one block within the COP domain.

It is recommended to read the System Requirement Specification before reading this document.

points-out the chosen block, where this interface control document will focus, and leave other interfaces as unexplored interfaces.



Figure 1 - SysML block diagram

## Interface identification and diagrams

This paragraph contains a identification of the limited system, which has been chosen to be described during this case work.

Figure 2, shows the chosen system interfaces.



Figure 2 - System interfaces

1. CCRT (Cross compatible radio - terminals): The interface between the different branches involved.
2. CCRC (Cross compatible radio - control): The interface to the headquarter, which provides and maintain the infrastructure and technology of this solution.

*Table 1* shows the overall setup of the interfaces.

|  |  |  |  |
| --- | --- | --- | --- |
| **Channel name** | **Source** | **Sink** | **Channel frequency** |
| CCRT | Bi-directional | | 380 - 921 MHz |
| CCRC | Bi-directional | | 380 - 921 MHz |

Table 1 - Interface overview

## CCRT and CCRC Interface

These two interfaces are treated as identical in this document since they, from a interface architects point-of-view, could be described the same way.

CCRT and CCRC will use the SINE solution , which is based TETRA technology, which is a wireless standard. TETRA is designed for use by government agencies, emergency services, police forces, fire departments, ambulance, rail transportation staff, and transport services.

TETRA is an ETSI standard [4] and works in a very similar way to GSM. The main differences are longer range and more bandwidth allocated for data.

### Type of interface

This interface complies with the TETRA communication standard [2]. It is a data transceiver interface, which will send or receive non-buffered data packages from the respective unit.

### Interface data elements and setup

The TETRA system is a Frequency Division Duplex (FDD) system. TETRA also uses FDMA/TDMA like GSM.

Modulation setup [3]:

* Digital modulation scheme: π/4 DQPSK (differential quadrature phase shift keying)
* Baud rate: 18000 sym/s
* Symbol maps: 2 bits/sym

Speech signals is the essential part of TETRA technology.

Speech channel [3]:

* Sampled at: 8 kbit/s
* Compressed with: ACELP (Adaptive Code Excited Linear Prediction).
* Data rate before channel coding: 4,567 kbit/s.
* Data rate after channel coding: 7,2 kbit/s.

A single slot consists of 255 usable symbols, the remaining time is used up with synchronisation sequences and turning on/off

### Address bus

NA

### Data bus

NA

### Memory Map

NA - Not a memory mapped interface

### Control registers

Read the TETRA ETSI standard [4]

### Status registers

Read the TETRA ETSI standard [4]

### Data registers

Read the TETRA ETSI standard [4]

### Hardware characteristics

Read the TETRA ETSI standard [4]

# Bibliography

1. **sikkerhedsnet.dk**.SINE-sekretariate, 2010.
2. **tetra-association.com**. The TETRA MoU Association Ltd, 2010.
3. **En.wikipedia.org/wiki/Terrestrial\_Trunked\_Radio**, Wikipedia, 2010
4. **etsi.org/website/Technologies/TETRA.aspx**. ETSI, 2010